# ID 50061

Number of programmed axes exceeds range within measuring block.
Description | In conjunction with the measurement function G100, several measurement types are available. These types can be selected via MDS or CNC program. The maximum number of programmed axes depends on selected measurement type . For detailed information on G100, see[FCT-C4], [PROG// Section: Measuring functions].
Response | Class | 4 | Movement stop.
Solution | Class | 6 | Only use maximum permissible number of axes in CNC program with selected measurement type or change measurement type.
Parameter | %1: | Current value [-]
Number of programmed axes.
%2: | Upper limit value [-]
Maximum permissible number of programmed axes of selected measurement type.
%3: | Current value [-]
Currently selected measurement type.
Error type | 1, Error message from NC program.