# ID 120486

Motion path exits workspace.
Description | Start point and target point of programmed motion path is outside active valid workspace. A workspace may not be exited by a tool centre point. A workspace may consist of a circular or polygonal area with constant third plane. See also FCT-C14.
Response | Class | 2 | Stop all axes immediately
Solution | Class | 6 | Take into account the defined activated workspaces
Parameter | %1: | Logical axis number [-]
Area Id number of exited workspace.
%2: | Incorrect value [0.1 µm or 0.0001°]
Start point of motion.
%3: | Upper limit value [0.1 µm or 0.0001°]
End point of motion.
%4: | Current value [0.1 µm or 0.0001°]
Intersection point of motion path on exiting the workspace.
%5: | Current value [0.1 µm or 0.0001°]
Error type | 1, Error message from NC program.