# Angle measurement

These cycles determine workpiece twist and the compensation value. The calculated value is transferred to the selected zero offset.

## Additional information

- Measure angle in X axis (C axis)
- Measure angle in Y axis (C axis)
- Measure angle between 2 drilled holes (C axis)
- Measure angle between pins (C axis)
- Measure angle between drilled hole and spigot (C axis)
- Measure angle between point in Y and drilled hole (C axis)
- Measure angle between point in Y and spigot (C axis)
- Measure angle between point in X and drilled hole (C axis)
- Measure angle between point in X and spigot (C axis)
- Measure angle in Z axis (A axis)
- Measure angle in Z axis (B axis)