# ID 50206

Spindle distance per cycle is 0.
Description | With turning function thread cutting (G33), current value of path per cycle is smaller than minimum value. For more information on turning functions see [PROG// Section: Turning functions].
Response | Class | 4 | Movement stop.
Solution | Class | 6 | Check current speed spindle, value should be > 0. Turning speed of spindle > 0 in NC program.
Parameter | %1: | Logical axis number [-]
Logical axis number of concerned spindle axis (P-AXIS-00016).
%2: | Current value [1µm/s or 0.001°/s]
Current spindle speed.
%3: | Current value [0.1 µm or 0.0001°]
Path per cycle.
%4: | Lower limit value [0.1 µm or 0.0001°]
Lower limit value for minimum path per cycle.
Error type | 1, Error message from NC program.