# ID 110579

P-AXIS-00511 may not be 0.
Description | Parameter P-AXIS-00511 was set to zero; this value is not permitted.
Response | Class | 1 | Error message output, value corrected to 1.
Solution | Class | 1 | Warning output, automatic correction of the value.
Parameter | %1: | Logical axis number [-]
Axis number
%2: | Incorrect value [-]
Set value of P-AXIS-00511.
%3: | Corrected value [-]
Corrected value of P-AXIS-00511.
Error type | 2, Error message on data transfer of parameter lists to controller.