# ID 50052

Probe already actuated.
Description | Before starting measurement motion with Measuring functions G100, check whether the measuring probe is currently active. The signal may not be enabled. For more information on Measuring functions G100 see [FCT-C4], [PROG// Section: Measuring functions].
Response | Class | 4 | Movement stop.
Solution | Class | 6 | Check measurement signal and signal level.
Parameter | %1: | Logical axis number [-]
Logical axis number of axis affected P-AXIS-00016.
%2: | Block number [-]
%3: | Current value [-]
Error type | 1, Error message from NC program.