# ID 110236

Leadscrew error compensation activated without compensation value list.
Description | The CNC detects an inconsistent parameterization regarding leadscrew error compensation. In an axis configuration list, leadscrew error compensation was activated via parameter P-AXIS-00175. The CNC now expects the information in which path and under which name a corresponding compensation value list can be found. To do this, the data in parameters P-STUP-00016, P-STUP-00017, P-STUP-00036 must be parameterized correctly in start-up list.

In the corresponding compensation value list, the parameters P-COMP-00001 and P-COMP-00020 must also be entered correctly for leadscrew error compensation.

Response | Class | 1 | CNC disables leadscrew error compensation.
Solution | Class | 7 | Check parameters P-STUP-00016 P-STUP-00017 P-STUP-00036 P-COMP-00001
P-COMP-00020 for consistent data.

If leadscrew error compensation is not desired, set parameter P-AXIS-00175 to the value 0.

Parameter | %1: | Logical axis number [-]
Parameter P-AXIS-00016 from an axis configuration list in which the leadscrew error compensation was activated via P-AXIS-00175.
Error type | 2, Error message by data transfer from parameter list into control device.