# ID 110118

At least one measurement method has to be defined.
Description | If the axis is marked as a measuring axis P-AXIS-00118, a measuring method must also be parameterized. The parameter P-AXIS-00117 is set to 1.
Response | Class | 1 | None.
Solution | Class | 1 | Depending on drive type P-AXIS-00020, at least one measuring signal has to be parameterized, or P-AXIS-00118 has to be set to zero.
Parameter | %1: | Logical axis number [-]
Logical axis number of concerned axis P-AXIS-00016.
%2: | Corrected value [-]
Current drive type @@P-AXIS-00020.
%3: |
Corrected parameter P-AXIS-00117.
Error type | 2, Error message by data transfer from parameter list into control device.