# ID 110286

Changing the counter channel requires restart of the control.
Description | The parameter P-AXIS-00041 defining the physical counter channel on I/O hardware cannot be changed while the CNC kernel is running. The new parameter value is not transferred, the previously active value remains valid.
Response | Class | 1 | None.
Solution | Class | 1 | Change the entry P-AXIS-00041 only in configuration mode or when the CNC is disabled.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected.
%2: | Current value [-]
Current value of P-AXIS-00041.
%3: | Corrected value [-]
Corrected value of P-AXIS-00041.
Error type | 2, Error message on data transfer of parameter lists to controller.