# ID 60141

Spindle is configured in too many channels.
Description | A spindle can only be configured in a certain number of channels at the same time. A spindle is configured in a channel by inserting a section spindel[].bezeichnung ... spindel[].log_achs_nr ... spindel[].plc_control ... spindel[].s_synch ...

spindel[].m3_synch ...

spindel[].m4_synch ...

spindel[].m5_synch ...

spindel[].m19_synch ...

spindel[].s_prozess_zeit ...

spindel[].m3_prozess_zeit ...

spindel[].m4_prozess_zeit ...

spindel[].m5_prozess_zeit ...

spindel[].m19_prozess_zeit ...

in the channel parameter list.

See also [CHAN//Section: Configuration of spindles].

Response | Class | 2 | Spindle changes to error state.
Solution | Class | 7 | Delete the entries or comments spindel[].bezeichnung ... spindel[].log_achs_nr ... spindel[].plc_control ... spindel[].s_synch ...

spindel[].m3_synch ...

spindel[].m4_synch ...

spindel[].m5_synch ...

spindel[].m19_synch ...

spindel[].s_prozess_zeit ...

spindel[].m3_prozess_zeit ...

spindel[].m4_prozess_zeit ...

spindel[].m5_prozess_zeit ...

spindel[].m19_prozess_zeit ...

in at least one channel parameter list.

Parameter | %1: | Logical axis number [-]
Logical axis number (P-AXIS-00016) of the spindle
%2: | Current value [-]
Number of channels in which the spindle is configured.
%3: | Limit value [-]
Maximum number of channels the spindle can be configured in.
Error type | -