# ID 110125

Maximum velocity for manual mode is not allowed to be 0.
Description | The maximum velocity P-AXIS-00213 with active manual operation mode is set to zero. The maximum velocity is set to default value.
Response | Class | 1 | None.
Solution | Class | 1 | Set maximum velocity for manual operation mode P-AXIS-00213 greater than 0.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [1µm/s or 0,001°/s]
Current maximum velocity P-AXIS-00213.
%3: | Corrected value [1µm/s or 0,001°/s]
Corrected maximum velocity P-AXIS-00213.
Error type | 2, Error message by data transfer from parameter list into control device.