# Default axis configuration in the channel after reset (P-CHAN-00179)

P-CHAN-00179 | Restore default axis configuration in the channel after reset
Description | This parameter defines whether the axis configuration is to be restored according to the channel parameter list after a reset in the NC channel.
Parameter | ax_default_config_after_reset
Data type | BOOLEAN
Data range | 0: Handling path axes as per P-CHAN-00075 and P-CHAN-00115 (default). 1: Restore basic configuration of axes after RESET according to channel parameter list.
Dimension | ----
Default value | 0
Remarks | It only makes sense to use this parameter if P-CHAN-00075 (reset_no_axis_to_axv) is assigned FALSE. See also P-AXIS-00251