# Output time M19 for positioning the spindle (P-AXIS-00523)

P-AXIS-00523 | Output time M19 for positioning the spindle
Description | The output time point of the spindle M-functions M03 and M04 for rotation is the start of the movement. On the other hand, when the spindle position moves, the CNC only outputs the M function M19 when the spindle reaches the target position.

When the value is set to 1, the M19 M function is output at the start of the spindle positioning analogue to the other spindle M functions. The M19 M function is acknowledged when the spindle reaches the target position.

Parameter | kenngr.spindle_m19_output_standard
Data type | BOOLEAN
Data range | 0/1
Axis types | S
Dimension |  | S: ----
Default value | 0
Drive types | ----
Remarks |