# Motion path limit (P-CHAN-00191)

P-CHAN-00191 | Motion path limit (path-dependent dynamic weighting)
Description | This parameter defines the upper motion path limit. The weighting factors of the current entries under the same index i are effective up to this limit.
Parameter | dynamic_weighting[i].path_limit
Data type | UNS32
Data range | 0 < path_limit < MAX(UNS32)
Dimension | 0.1 µm or 0.0001º
Default value | 0
Remarks | The maximum index i in the table has a special importance: Here the upper limit of the motion path corresponds to the machine-specific maximum contour path. Therefore, this area is valid for all motion blocks which are not covered by the path distance limits of the lower areas of the table.