# ID 70510

With active Volumetric Compensation changing the compensation axis is not permitted.
Description | Axes involved in Volumetric Compensation can be changed via a write access to the global variables V.G.VOLCOMP[i].X/Y/Z/A/B/C. However, this change is not allowed while the respective compensation is still enabled.
Response | Class | 3 | Program abort.
Solution | Class | 6 | Disable compensation before changing the axis configuration.
Parameter | %1: | Compensation index [-]
ID of Volumetric Compensation
%2: | Axis name [-]
%3: | Logical axis number [-]
Previous axis number of the axis used
%4: | Logical axis number [-]
Axis number of the new axis to be used
%5: | Block number [-]
Error type | 11, Error message from position controller.