# ID 70662

Calculated metric position out of permissible range.
Description | The position set by the NC program is outside the permissible value range. (+- 214.746m). See Setting an axis position in the channel (SET_POSITION)
Response | Class | 7 | Controlled halt of the axis, the control loop is closed.
Solution | Class | 6 | Check and modify the position to be set. Select a position that is within the permitted metric value range.
Parameter | %1: | Logical axis number [-]
Logical axis number Axis parameters of the axis affected
%2: | Error value [-]
Specified axis position
%3: | Upper limit value [-]
Maximum possible axis position
%4: | Lower limit value [-]
Minimum possible axis position
Error type | 11, Error message from position controller.