# Restore coupling after program end (P-CHAN-00105)

P-CHAN-00105 | Restore coupling after program end (synchronous operation)
Description | An active axis coupling (synchronous operation) is deselected at NC program end (#DISABLE AXLINK) if it is not ended explicitly in the NC program. Set this parameter to 1 if the axis coupling is to be reactivated automatically in the following NC program.
Parameter | synchro_data.preserve_coupling_after_prog_end
Data type | BOOLEAN
Data range | 0/1
Dimension | ----
Default value | 0
Remarks | This parameter may only be used if all axes participating in the coupling exist in the basic configuration of the NC channel.