# ID 60303

Offset angle for thread cutting is outside modulo area.
Description | For thread cutting G33 an offset angle S.OFFSET was specified greater than the spindle modulo range. The thread offset angle is only required for multi-start threads. See [PROG// Section: Thread cutting with endlessly rotating spindle] Example:

G33 Z48 K1.5 S.OFFSET=500

Correct:

G33 Z48 K1.5 S.OFFSET=180

Response | Class | 7 | Stop of axis and abortion of CNC program
Solution | Class | 6 | Correct CNC program
Parameter | %1: |
Logical axis number P-AXIS-00016 of concerned axis
%2: | Current value [0.1 µm or 0.0001°]
%3: | Limit value [0.1 µm or 0.0001°]
Lower modulo limit P-AXIS-00127 of the axis
%4: | Limit value [0.1 µm or 0.0001°]
Upper modulo limit P-AXIS-00126 of the axis
Error type | 1, Error message from NC program.