# Parameters

Input parameters | Description
@P33 | Permissible tolerance of the measuring points to determine tool breakage. If this value is exceed, it is evaluated as a tool breakage. (default = 0.5)
@P37 | Permissible tolerance of the measuring points to determine tool wear. (default = 0.1) It the tolerance is too small, it may result in unnecessary machine stops.
@P67 | Radius offset (lateral offset when probing) Only positive values are permissible. Set the offset according to the tool measurement. (default = 0)
@P70 | 0 (default) = warning when tool is worn, 1 = stop when tool is worn
@P71 | 0 (default) = warning when tool breaks, 1 = stop when tool breaks

It is recommended using the Syntax check.to verify whether the input parameters have been correctly assigned.