# ID 60247

SGN64-overflow in virtual master position with gear factor.
Description | The virtual master position with gear factor compensation is outside the permissible numerical range. The position value must be smaller than 9.223.372.036.854.775.807 (maximum signed 8 byte number).
Response | Class | 5 | Abrupt axis stop, feed hold for the other axes.
Solution | Class | 6 | Correct virtual master position and do nc reset.
Error type | -