# Description

These cycles are used to determine the precise position, orientation and zero position using a touch probe or a reference tool.

The values determined are written to a subroutine.

The measurement results are on V.CYC variables (output variables) and can be processed in the post files.

## Additional information

- General
- Parameters
- Configuration file
- Pre- and post-files
- General cycle process