# ID 1599

Not enough block motion path for position controlled stop.
Description | After activation of measurement signal via measuring probe, residual path P-CHAN-00030 defined in channel parameter list is reduced with active function edge bending. The residual path available of current active channel block at this moment must be greater than P-CHAN-00030. Depending on setting of P-CHAN-00029 the residual path is declined by one or more channel motion blocks. Braking distance after activation of probing sensor depends on dynamic settings in axes machine data!

For further informations see PROG//Section: Edge bending.

Response | Class | 6 | Program execution stop.
Solution | Class | 7 | Check whether there is sufficient residual path available in the NC program after activating the measuring probe. Increase residual path or, if possible, reduce the value of channel parameter P-CHAN-00030.
Parameter | %1: | Expected value [0.1 µm or 0.0001°]
Current necessary braking distance.
%2: | Current value [0.1 µm or 0.0001°]
Current remaining movement residual path.
Error type | 1, Error message from NC program.