# ID 110385

Acceleration minimum is smaller than minimum permissible value.
Description | Minimum acceleration limit P-AXIS-00010 of the curve-controlled acceleration was specified too high. This value must not be higher than the minimum acceleration.
Response | Class | 1 |
Solution | Class | 1 |
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Current value [1µm/s or 0.001°/s]
P-AXIS-00010
%3: | Limit value [1µm/s or 0.001°/s]
%4: | Incorrect value [1µm/s or 0.001°/s]
P-AXIS-00010
Error type | 2, Error message on data transfer of parameter lists to controller.