# ID 20007

Spindle speed is 0.
Description | With thread tapping G63, the spindle speed must not be zero (nil). Example: Wrong: N10 G63 Z10 F300 S0 Correct:

N10 G63 Z10 F300 S17

Response | Class | 2 | Abort NC program processing. .
Solution | Class | 3 | Match spindle speed, feed rate and selected pitch PROG//Section: Tapping.
Parameter | %1: | Logical axis number [-]
Error type | 1, Error message from NC program.