# ID 20113

Double-programmed TRC transition block mode.
Description | More than one G function from the group of TRC transition types (G25/G26) has been programmed in the same NC block. Example: Wrong: N10 G00 X0 Y0 Z0 G42 N20 G25 G25

:

N1000 M30

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. Remove the inadmissible G function.
Parameter | %1: | Error value [-]
Number of the inadmissible programmed G function
Error type | 1, Error message from NC program.