# ID 110385

The value of a_min is smaller as the lower limit value.
Description | Minimum acceleration limit P-AXIS-00010 of the characteristic-guided acceleration was specified too large. This value must not be above the minimum acceleration.
Response | Class | 1 |
Solution | Class | 1 |
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Current value [1µm/s or 0,001°/s]
P-AXIS-00010
%3: | Limit value [1µm/s or 0.001°/s]
%4: | Error value [1µm/s or 0,001°/s]
P-AXIS-00010
Error type | 2, Error message by data transfer from parameter list into control device.