# ID 110589

Parameter P-AXIS-00519 can only be used for spindles.
Description | Parameter P-AXIS-00519 was set for an axis other than a spindle (see P-AXIS-00018).
Response | Class | 1 | Warning output, P-AXIS-00519 is corrected to zero.
Solution | Class | 1 | P-AXIS-00519 for non spindle axes shall be set to zero (nil).
Parameter | %1: | Logical axis number [-]
Log. Axis number (P-AXIS-00016)
%2: | Current value [-]
Axis type (P-AXIS-00018)
%3: | Error value [-]
Current value of P-AXIS-00519
%4: | Corrected value [-]
Corrected value of P-AXIS-00519
Error type | 2, Error message by data transfer from parameter list into control device.