# Parameters

Cycle parameters | Description
@P2 | Drilled hole diameter
@P7 (optional) | Zero offset to be described (TCS) G54 to G59 Input without address “G” If not specified, then measurement only but no write function
@P9 (optional) | Shift the measuring point along the X axis
@P10 (optional) | Shift the measuring point along the Y axis
@P13 (optional) | Security distance for pre-positioning
@P17 | Pre-position along the X axis above the drilled holes
@P18 | Pre-position along the Y axis above the drilled holes
@P19 | Pre-position along the Z axis above the drilled holes
@P33 (optional) | Crossover range [mm, inch] Default value = 5

If @P13 is not specified, the entire measuring section is traversed at the measuring feedrate.