# ID 13408

Zero point is not defined or incorrectly defined @P7. Values 54-59 are allowed.
Description | No origin is defined, or a wrong value is set.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Define the zero point at cycle call with the parameter @P7. Valid numbers are 54 to 59.
Error type | 1, Error message from NC program.