# ID 294539

Invalid DSE measuring channel.
Description | The denoted DSE measuring channel is not valid.
Response | Class | 7 | Stop axis motion immediately.
Solution | Class | 6 | Check measuring channel. Do reset.
Parameter | %1: | Current value [-]
Actual value of the measuring channel.
%2: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%3: | Drive type [-]
Drive type of the axis.
%4: | NC block number [-]
NC block number.
Error type | 11, Error message from position controller.