# ID 250009

Number of unacknowledged BROADCAST SIGNAL/WAIT exceeds limit.
Description | Too many BROADCAST #SIGNAL or #WAIT were programmed,and they have not yet been acknowledged. The memory limit is reached.
Response | Class | 3 |
Solution | Class | 6 | When programming, make sure that the limits documented in [SYSP] are not exceeded. Modify the NC programs accordingly.
Parameter | %1: | Limit value [-]
Maximum number of open #SIGNAL / #WAIT signals of the controller.
%2: | Current value [-]
Number of open #SIGNAL / #WAIT .
%3: | Limit value [-]
%4: | Current value [-]
Error type | -