# ID 50894

Axis must not be released when programmed axis coupling is active.
Description | An attempt is made to release an axis by axis exchange command when a coupling activated by #GEAR LINK [] is active. This is not permissible.
Response | Class | 6 |
Solution | Class | 4 |
Parameter | %1: | Logical axis number [-]
%2: | Error value [-]
State of coupling via #GEAR LINK[]
Error type | 1, Error message from NC program.