# ID 20642

M19 not allowed during active constant cutting speed
Description | With the selection of spindle positioning (M19, it is detected that constant cutting speed (G96) is still active.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and change NC program. Before selecting spindle positioning with M19, explicitly deselect the constant cutting speed (G96) with G97.
Error type | 1, Error message from NC program.