# ID 60262

Spindle axis exchanged. Action cannot be executed.
Description | The job sent to the spindle cannot be executed since the axis was replaced from the spindle interpolator. First replace the spindle axis. See also [[PROG// Section: Releasing/requesting spindle axes].
Response | Class | 6 | Immediate stop of the axis
Solution | Class | 6 | If the command was issued by the PLC to the spindle the command content was wrong or the command was sent at the wrong time to the spindle. Possible reasons are:

- Programming error in the PLC. See also [HLI// Section: External spindle command].
- Wrong version of the PLC library used to command the job.
- No synchronization between PLC and CNC.

Parameter | %1: |
Logical axis number of the spindle axis.
Error type | 1, Error message from NC program..