# ID 120482

A full circle without end point is required for a circular area.
Description | A circular area consists of a linear block as starting point and a circular block as circular description. A circular block must be a programmed full circle since areas can only consist of a full circle. See also [PROG// Monitoring the workspace and protection space]

Example with error:

%circular area

N10 #CONTROL AREA BEGIN [ID51 PROT CIRC MIN_EXCU…

N20 G01 X150 Y200 F10000

N30 G03 G162 I50 J0 X250 Y200 F10000

N40 #CONTROL AREA END

N50 M30

Corrected example:

%circular area

N10 #CONTROL AREA BEGIN [ID51 PROT CIRC MIN_EXCU…

N20 G01 X150 Y200 F10000 (start point)

N30 G03 G162 I70 J150

N40 #CONTROL AREA END

N50 M30

Response | Class | 2 | Abort NC program processing.
Solution | Class | 6 | Check and modify the area definition in the NC program.
Parameter | %1: | Identification number [-]
Area ID
%2: | Initial value [0.1 10^-3 mm or ø]
Starting point for the circle description.
%3: | Final value [0.1 10^-3 mm or ø]
Target point for the circle description.
Error type | 1, Error message from NC program.