# Position correction

In some applications the manual operation mode interface is used for position correction. So, in general, the velocities and accelerations which are greater than the maximum limits must also be set. The following parameters permit the setting of specific dynamic values for manual operation mode.

## Additional information

- Velocity during position correction (P-AXIS-00365)
- Acceleration during position correction (P-AXIS-00366)