# ID 40097

System error: More configured spindles notified than axes configured.
Description | During the start-up phase of the PLC application a check is made how many spindles were configured. They are axes in which the axis type is defined by ACHSTYP_SPINDEL in the axis parameter list (P-AXIS-00008) of the motion controller. If this error message appears, more configured spindles were signalled than there are axes. However, the number of spindles is always less than or equal to the number of axes.
Response | Class | - | No link is made to the motion controller.
Solution | Class | - | Please contact your motion control supplier.
Error type | -