# ID 110512

Homing on encoder overflow and homing on zero pulse can not be active at the same time.
Description | Homing to encoder overflow (see P-AXIS-00294) and homing to zero pulse search (see P-AXIS-00386) have been activated simultaneously.
Response | Class | 1 | Error message output, reference to encoder overflow (P-AXIS-00294) is disabled.
Solution | Class | 1 | Set either P-AXIS-00294 or P-AXIS-00386 to zero (nil).
Parameter | %1: | Logical axis number [-]
Log. Axis number (see also P-AXIS-00016).
%2: | Current value [-]
Value of P-AXIS-00386.
%3: | Current value [-]
Value of P-AXIS-00294.
%4: | Corrected value [-]
Corrected value of P-AXIS-00294.
Error type | 2, Error message by data transfer from parameter list into control device.