# ID 70182

Invalid logical axis number for plane compensation.
Description | The logical axis number of the first or second master axis for plane compensation is invalid, since its value is specified as zero or does not exist. Axes whose actual positions influence the compensation value are named master axes. The function is switched off for the specified axis (see P-AXIS-00174).

See also [FCT-C5// Section: Plane compensation]

Response | Class | 7 | Closed-loop controlled axis stop. Plane compensation is turned off for the affected axis.
Solution | Class | 7 | Correct logical axis numbers of master axes, see P-COMP-00014 and P-COMP-00015
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis, see P-AXIS-00016
%2: | Logical axis number [-]
Logical axis number of first master axis, see P-COMP-00014
%3: | Logical axis number [-]
Logical axis number of second master axis, see P-COMP-00015
Error type | 2, Error message by data transfer from parameter list into control device.