# ID 70335

Before activating distance control the command height must be specified.
Description | Before distance control is activated, specify the command height of the workpiece surface SET_POS. Example: Z [DIST_CTRL ON Before activating distance control the command height must be specified.] See [FCT-M3// Section: Specifying the workpiece surface]
Response | Class | 7 | Immediate axis stop. Distance control is not enabled.
Solution | Class | 6 | Specify the set height of the workpiece surface SET_POS
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected
%2: | Block number [-]
Block number in the NC program where the error occurred.
Error type | 11, Error message from position controller.