# Minimum segment length for block segmentation (P-CHAN-00140)

P-CHAN-00140 | Minimum segment length for block segmentation (HSC)
Description | This parameter defines the minimum segment length for block segmentation due to the dynamics in the contour. Lower values lead to improved use of the dynamics but also to a larger number of blocks.
Parameter | hsc.gen.min_segment_length
Data type | UNS32
Data range | 1 ... MAX(UNS32)
Dimension | 0.1µm
Default value | 200
Remarks |