# ID 120173

Missing pitch axis.
Description | With turning function thread cutting (G33), the pitch axis which is programmed via I, J or K parameter must be available as main axis in CNC channel. For more information on turning functions see [PROG// Section: Turning functions].
Response | Class | 2 | Program execution stop.
Solution | Class | 6 | Check axis configuration, depending on programmed I, J, or K parameters, main axis 1, 2 or 3 must be available in CNC channel.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of pitch axis.
Error type | 1, Error message from NC program.