# ID 70312

Activation of leadscrew error compensation not possible since axis is not homed.
Description | The axis must be homed in order to activate leadscrew error compensation. See FCT-C5]// Section: Leadscrew error compensation]
Response | Class | 1 | Warning, lead screw error compensation remains inactive until axis is homed
Solution | Class | 1 | Home the axis (see [FCT-M1]) If an absolute measurement system is used, parameter P-AXIS-00014 can be set to 1 to mark the homing of the axis.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected
%2: | Error value [-]
TRUE, if axis is homed
Error type | 11, Error message from position controller.