# ID 110678

Changing of P-AXIS-00795 requires restart of the control.
Description | A change in the parameter P-AXIS-00795 pos_lag_model.pos_lag_batch_num requires a controller restart.
Response | Class | 1 | Output of warning; adopt the new value.
Solution | Class | 1 | The new value is adopted; a controller restart is required.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected.
%2: | Current value [-]
Current value for P-AXIS-00795.
%3: | Corrected value [-]
New value for P-AXIS-00795.
Error type | -