# ID 110569

Positive absolute ACS manual mode limit is smaller than negative limit.
Description | The absolute positive movement limit P-AXIS-00493 for the movement range in active manual operation mode is smaller than the negative software limit switch P-AXIS-00492. The Monitoring is disabled.
Response | Class | 1 | None.
Solution | Class | 1 | Set positive motion limit P-AXIS-00493 greater than the negative motion limit P-AXIS-00492.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [-]
Current value for positive offset limit P-AXIS-00493.
%3: | Current value [-]
Current value of negative offset limit @@P-AXIS-00492.
%4: | Corrected value [-]
Corrected value for positive offset limit P-AXIS-00493.
%5: | Corrected value [-]
Corrected value for negative offset limit P-AXIS-00492.
Error type | 2, Error message by data transfer from parameter list into control device.