# Process (internal cycle)

The internal cycle process can be described as follows:

1. Pre-position above the measuring surface in Y and then measure in Z direction.
2. After clearance, the device moves back to the starting point.
3. Pre-position in front of the measuring surface in Z and then measure in Y direction.
4. After clearance, the device moves back to the starting point.
5. Description of selected zero offset.