# ID 60262

Spindle axis is exchanged. Action cannot be executed.
Description | The job sent to the spindle cannot be executed since the axis was replaced from the spindle interpolator. First replace the spindle axis. See also [PROG// Section: Releasing/requesting spindle axes].
Response | Class | 6 | Stop axis immediately
Solution | Class | 6 | If the command was transferred by the PLC to the spindle, this error indicates that the command in the PLC was incorrect or the command was sent to the spindle at the wrong time. Possible reasons are:

- Programming error in the PLC. See also [HLI// Section: External spindle command].
- Wrong version of the PLC library used to command the job.
- No synchronisation between PLC and CNC.

Parameter | %1: |
Logical axis number of the spindle axis.
Error type | 1, Error message from NC program..