# ID 21579

Invalid setting of H function by tube profile parameter.
Description | The parameter setting of the tube profile processing #CYL[] function in the machine data record contains incorrect M/H code numbers. Either the M/H code exceeds maximum permissible value or an internally assigned M code number was used (e.g. M30 -> program end code).

Invalid parameter setting leads to deactivation of specific M/H code output.

Response | Class | 1 | Abort NC program processing.
Solution | Class | 1 | Check and correct parameter settings of channel machine data tube_profile.techno_nr_rnd_on, tube_profile.techno_nr_rnd_off
Parameter | %1: | Current value [-]
Current invalid M/H number
%2: | Limit value [-]
Maximum permissible M/H code number
%3: | Corrected value [-]
Corrected M/H code number
Error type | 2, Error message by data transfer from parameter list into control device.