# ID 110067

Axis data for gear step incomplete.
Description | The machine parameter list was not completely initialized. This can just happen, if the parameter set of an axis is passed in binary form to the CNC.
Response | Class | 3 |
Solution | Class | 7 |
Parameter | %1: | Logical axis number [-]
%2: | Error value [-]
incorrect bit
Error type | 2, Error message by data transfer from parameter list into control device.