# ID 110145

Positive manual mode offset limit negative.
Description | The positive offset limit P-AXIS-00138 for the positive movement range with active manual operation mode is less than 0. The offset limit is corrected according to specific default value.
Response | Class | 1 | None.
Solution | Class | 1 | Set positive offset limit P-AXIS-00138 greater than 0.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Current value [-]
Current value P-AXIS-00138.
%3: | Current value [-]
Corrected value P-AXIS-00138.
%4: | Corrected value [-]
%5: | Corrected value [-]
Error type | 2, Error message by data transfer from parameter list into control device.